Real time clock (RTC\_arduino)

* With the Arduino unpowered, wire the “Real-time clock module as follows”.
* You’ll need to install the library from <https://github.com/adafruit/RTCLib>
* To observe data open serial monitor and set baud rate to 115200.

|  |  |  |
| --- | --- | --- |
| Pin | Function | Attached to |
| 5V | To power RTC | Analog 5V |
| GND | Ground | GND |
| SCL | Not sure | Analog 5 (A5) |
| SDA | Not sure | Analog 4 (A4) |

